(kicad_pcb (version 3) (host pcbnew "(2013-mar-13)-testing")
  (general
    (links 109)
    (no_connects 0)
    (area 74.7395 72.588 143.9535 105.029001)
    (thickness 1.6)
    (drawings 24)
    (tracks 395)
    (zones 0)
    (modules 41)
    (nets 42)
  )
  (page A4)
  (layers
    (15 F.Cu signal)
    (0 B.Cu signal)
    (16 B.Adhes user)
    (17 F.Adhes user)
    (18 B.Paste user)
    (19 F.Paste user)
    (20 B.SilkS user)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (24 Dwgs.User user)
    (25 Cmts.User user)
    (26 Eco1.User user)
    (27 Eco2.User user)
    (28 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.508)
    (trace_clearance 0.1778)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.762)
    (via_min_drill 0.381)
    (user_via 1.524 0.762)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (pad_to_paste_clearance -0.075)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 284721153)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3.3V)
  (net 2 /ACTLED)
  (net 3 /LNKLED)
  (net 4 /NICAVDD)
  (net 5 /PMODE0)
  (net 6 /RCT)
  (net 7 /RD+)
  (net 8 /RSVD)
  (net 9 /RSVD5)
  (net 10 /RX-)
  (net 11 /RXN)
  (net 12 /RXP)
  (net 13 /SCK)
  (net 14 /SI)
  (net 15 /SO)
  (net 16 /TCT)
  (net 17 /TXN)
  (net 18 /TXP)
  (net 19 /XI)
  (net 20 /XO)
  (net 21 /nCS)
  (net 22 /nINT)
  (net 23 /nRST)
  (net 24 GND)
  (net 25 N-000001)
  (net 26 N-0000014)
  (net 27 N-0000015)
  (net 28 N-000002)
  (net 29 N-000003)
  (net 30 N-0000031)
  (net 31 N-0000033)
  (net 32 N-0000034)
  (net 33 N-0000035)
  (net 34 N-0000036)
  (net 35 N-0000037)
  (net 36 N-0000038)
  (net 37 N-0000039)
  (net 38 N-000004)
  (net 39 N-0000040)
  (net 40 N-000005)
  (net 41 N-000006)
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.254)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
    (add_net +3.3V)
    (add_net /ACTLED)
    (add_net /LNKLED)
    (add_net /NICAVDD)
    (add_net /PMODE0)
    (add_net /RCT)
    (add_net /RD+)
    (add_net /RSVD)
    (add_net /RSVD5)
    (add_net /RX-)
    (add_net /RXN)
    (add_net /RXP)
    (add_net /SCK)
    (add_net /SI)
    (add_net /SO)
    (add_net /TCT)
    (add_net /TXN)
    (add_net /TXP)
    (add_net /XI)
    (add_net /XO)
    (add_net /nCS)
    (add_net /nINT)
    (add_net /nRST)
    (add_net GND)
    (add_net N-000001)
    (add_net N-0000014)
    (add_net N-0000015)
    (add_net N-000002)
    (add_net N-000003)
    (add_net N-0000031)
    (add_net N-0000033)
    (add_net N-0000034)
    (add_net N-0000035)
    (add_net N-0000036)
    (add_net N-0000037)
    (add_net N-0000038)
    (add_net N-0000039)
    (add_net N-000004)
    (add_net N-0000040)
    (add_net N-000005)
    (add_net N-000006)
  )
  (module HR911105_RJ45 (layer F.Cu) (tedit 52C49C95)
    (at 86.1695 89.789 270)
    (tags HR911105_RJ45)
    (fp_text reference J2 (at -0.0508 6.59892 270) (layer F.SilkS) hide)
    (fp_text value HR911105_RJ45 (at 0.14224 -0.1016 270) (layer F.SilkS) hide)
    (pad Hole thru_hole circle (at 5.69976 -0.24892 270) (size 3.59918 3.59918) (drill 3.2512)
      (layers *.Cu *.SilkS *.Mask)
    )
    (pad Hole thru_hole circle (at -5.69976 -0.20066 270) (size 3.59918 3.59918) (drill 3.2512)
      (layers *.Cu *.SilkS *.Mask)
    )
    (pad 1 thru_hole rect (at -4.39928 -6.55066 270) (size 1.778 1.778) (drill 0.89916)
      (layers *.Cu *.Mask F.SilkS)
      (net 18 /TXP)
    )
    (pad 2 thru_hole circle (at -3.2004 -9.10082 270) (size 2.032 2.032) (drill 0.89916)
      (layers *.Cu *.Mask F.SilkS)
      (net 17 /TXN)
    )
    (pad 3 thru_hole circle (at -1.89992 -6.55066 270) (size 2.032 2.032) (drill 0.89916)
      (layers *.Cu *.Mask F.SilkS)
      (net 7 /RD+)
    )
    (pad 4 thru_hole circle (at -0.59944 -9.10082 270) (size 2.032 2.032) (drill 0.89916)
      (layers *.Cu *.Mask F.SilkS)
      (net 16 /TCT)
    )
    (pad 5 thru_hole circle (at 0.59944 -6.55066 270) (size 2.032 2.032) (drill 0.89916)
      (layers *.Cu *.Mask F.SilkS)
      (net 6 /RCT)
    )
    (pad 6 thru_hole circle (at 1.89992 -9.10082 270) (size 2.032 2.032) (drill 0.89916)
      (layers *.Cu *.Mask F.SilkS)
      (net 10 /RX-)
    )
    (pad 7 thru_hole circle (at 3.2004 -6.55066 270) (size 2.032 2.032) (drill 0.89916)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 8 thru_hole circle (at 4.39928 -9.10082 270) (size 2.032 2.032) (drill 0.89916)
      (layers *.Cu *.Mask F.SilkS)
    )
    (pad 9 thru_hole circle (at -6.64972 3.79984 270) (size 2.032 2.032) (drill 1.00076)
      (layers *.Cu *.SilkS *.Mask)
      (net 25 N-000001)
    )
    (pad 10 thru_hole circle (at -4.09956 3.79984 270) (size 2.032 2.032) (drill 1.00076)
      (layers *.Cu *.SilkS *.Mask)
      (net 3 /LNKLED)
    )
    (pad 11 thru_hole circle (at 4.09956 3.79984 270) (size 2.032 2.032) (drill 1.00076)
      (layers *.Cu *.SilkS *.Mask)
      (net 2 /ACTLED)
    )
    (pad 12 thru_hole circle (at 6.64972 3.79984 270) (size 2.032 2.032) (drill 1.00076)
      (layers *.Cu *.SilkS *.Mask)
      (net 28 N-000002)
    )
    (pad 0 thru_hole circle (at -7.65048 -3.2004 270) (size 2.54 2.54) (drill 1.6002)
      (layers *.Cu *.SilkS *.Mask)
      (net 24 GND)
    )
    (pad 0 thru_hole circle (at 7.74954 -3.2004 270) (size 2.54 2.54) (drill 1.6002)
      (layers *.Cu *.SilkS *.Mask)
      (net 24 GND)
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3DF8C)
    (at 119.0625 87.0585 180)
    (attr smd)
    (fp_text reference C1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 18pF (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 20 /XO)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E032)
    (at 98.1075 92.964 180)
    (attr smd)
    (fp_text reference C2 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 22nF (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 16 /TCT)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3DFA1)
    (at 118.999 94.6785 180)
    (attr smd)
    (fp_text reference C3 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 18pF (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 19 /XI)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E048)
    (at 98.1075 87.884 180)
    (attr smd)
    (fp_text reference C4 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 6.8nF (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 12 /RXP)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 7 /RD+)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E043)
    (at 98.1075 89.535 180)
    (attr smd)
    (fp_text reference C5 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 6.8nF (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 11 /RXN)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 10 /RX-)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module c_tant_A (layer F.Cu) (tedit 52C3DF81)
    (at 127.0635 84.5185 180)
    (descr "SMT capacitor, tantalum size A")
    (fp_text reference C6 (at 0.0254 -1.2954 180) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.27 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.37414 0 180) (size 1.95072 1.50114)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at -1.37414 0 180) (size 1.95072 1.50114)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (model smd/capacitors/c_tant_A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3DF9C)
    (at 116.3955 93.599 90)
    (attr smd)
    (fp_text reference C7 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3DFF4)
    (at 109.728 98.044 90)
    (attr smd)
    (fp_text reference C8 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 4.7uF (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 33 N-0000035)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3DFF0)
    (at 111.379 98.044 90)
    (attr smd)
    (fp_text reference C9 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 10nF (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 31 N-0000033)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E036)
    (at 100.838 92.964)
    (attr smd)
    (fp_text reference C10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 10nF (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 6 /RCT)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module c_tant_A (layer F.Cu) (tedit 52C3E020)
    (at 99.8855 98.4885)
    (descr "SMT capacitor, tantalum size A")
    (fp_text reference C11 (at 0.0254 -1.2954) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.27) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.37414 0) (size 1.95072 1.50114)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (pad 2 smd rect (at -1.37414 0) (size 1.95072 1.50114)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (model smd/capacitors/c_tant_A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3DFFD)
    (at 110.236 95.885)
    (attr smd)
    (fp_text reference C12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E00A)
    (at 108.077 97.2185 90)
    (attr smd)
    (fp_text reference C13 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E00E)
    (at 106.426 97.2185 90)
    (attr smd)
    (fp_text reference C14 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E01B)
    (at 103.505 93.7895 90)
    (attr smd)
    (fp_text reference C15 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E068)
    (at 103.505 90.9955 90)
    (attr smd)
    (fp_text reference C16 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E062)
    (at 103.505 88.2015 270)
    (attr smd)
    (fp_text reference C17 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED-0805 (layer F.Cu) (tedit 52C3DFB9)
    (at 123.19 95.377 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -1.27 180) (layer F.SilkS) hide)
    (fp_text value LED_RED (at 0 1.27 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 38 N-000004)
    )
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 26 N-0000014)
    )
  )
  (module LED-0805 (layer F.Cu) (tedit 52C3DFBF)
    (at 123.1265 97.9805 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at 0 -1.27 180) (layer F.SilkS) hide)
    (fp_text value LED_GRN (at 0 1.27 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 27 N-0000015)
    )
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 3 /LNKLED)
    )
  )
  (module LED-0805 (layer F.Cu) (tedit 52C3DFB4)
    (at 123.19 92.9005 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D3 (at 0 -1.27 180) (layer F.SilkS) hide)
    (fp_text value LED_RED (at 0 1.27 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 41 N-000006)
    )
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 29 N-000003)
    )
  )
  (module LED-0805 (layer F.Cu) (tedit 52C3DFAD)
    (at 123.2535 90.297 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D4 (at 0 -1.27 180) (layer F.SilkS) hide)
    (fp_text value LED_YLW (at 0 1.27 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 40 N-000005)
    )
    (pad 2 smd rect (at 1.04902 0 180) (size 1.19888 1.19888)
      (layers F.Cu F.Paste F.Mask)
      (net 2 /ACTLED)
    )
  )
  (module pin_strip_8 (layer F.Cu) (tedit 52C3DFCC)
    (at 119.6975 81.4705)
    (descr "Pin strip 8pin")
    (tags "CONN DEV")
    (fp_text reference J1 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value HEADER_8 (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -8.89 0) (size 1.524 2.19964) (drill 1.00076)
      (layers *.Cu *.Mask F.SilkS)
      (net 23 /nRST)
    )
    (pad 2 thru_hole oval (at -6.35 0) (size 1.524 2.19964) (drill 1.00076)
      (layers *.Cu *.Mask F.SilkS)
      (net 22 /nINT)
    )
    (pad 3 thru_hole oval (at -3.81 0) (size 1.524 2.19964) (drill 1.00076)
      (layers *.Cu *.Mask F.SilkS)
      (net 14 /SI)
    )
    (pad 4 thru_hole oval (at -1.27 0) (size 1.524 2.19964) (drill 1.00076)
      (layers *.Cu *.Mask F.SilkS)
      (net 15 /SO)
    )
    (pad 5 thru_hole oval (at 1.27 0) (size 1.524 2.19964) (drill 1.00076)
      (layers *.Cu *.Mask F.SilkS)
      (net 13 /SCK)
    )
    (pad 6 thru_hole oval (at 3.81 0) (size 1.524 2.19964) (drill 1.00076)
      (layers *.Cu *.Mask F.SilkS)
      (net 21 /nCS)
    )
    (pad 7 thru_hole oval (at 6.35 0) (size 1.524 2.19964) (drill 1.00076)
      (layers *.Cu *.Mask F.SilkS)
      (net 1 +3.3V)
    )
    (pad 8 thru_hole oval (at 8.89 0) (size 1.524 2.19964) (drill 1.00076)
      (layers *.Cu *.Mask F.SilkS)
      (net 24 GND)
    )
    (model walter/pin_strip/pin_strip_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3DFD3)
    (at 111.6965 83.8835)
    (attr smd)
    (fp_text reference R1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 23 /nRST)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3DF86)
    (at 123.5075 84.5185 270)
    (attr smd)
    (fp_text reference R2 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 21 /nCS)
    )
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E03B)
    (at 98.1075 91.2495 180)
    (attr smd)
    (fp_text reference R3 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 10 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 16 /TCT)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E054)
    (at 101.981 86.233 90)
    (attr smd)
    (fp_text reference R4 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 49.9 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 18 /TXP)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E04D)
    (at 100.33 86.233 90)
    (attr smd)
    (fp_text reference R5 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 49.9 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (pad 2 smd rect (at 0.762 0 90) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 17 /TXN)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E025)
    (at 98.1075 96.52 180)
    (attr smd)
    (fp_text reference R6 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 28 N-000002)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E02B)
    (at 98.1075 94.742 180)
    (attr smd)
    (fp_text reference R7 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 25 N-000001)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3DF92)
    (at 116.3955 90.8685 270)
    (attr smd)
    (fp_text reference R8 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 1M (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 20 /XO)
    )
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 19 /XI)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E058)
    (at 100.838 88.519)
    (attr smd)
    (fp_text reference R9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 82 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 6 /RCT)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 12 /RXP)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E016)
    (at 104.013 95.9485 180)
    (attr smd)
    (fp_text reference R10 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 12.4k (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 39 N-0000040)
    )
    (pad 2 smd rect (at 0.762 0 180) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3E05D)
    (at 100.838 90.3605)
    (attr smd)
    (fp_text reference R11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 82 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 11 /RXN)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 6 /RCT)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3DFEB)
    (at 113.03 98.044 270)
    (attr smd)
    (fp_text reference R12 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 9 /RSVD5)
    )
    (pad 2 smd rect (at 0.762 0 270) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module r_cat16-4 (layer F.Cu) (tedit 52C49B50)
    (at 127.4445 87.5665 270)
    (descr "SMT resistor net, Bourns CAT16 series, 4 way")
    (fp_text reference RP3 (at 0 -2.10058 270) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 1.99898 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.762 0.39878 270) (size 0.762 0.4318)
      (layers F.Cu F.Paste F.Mask)
      (net 41 N-000006)
    )
    (pad 7 smd rect (at -0.762 0.39878 270) (size 0.762 0.4318)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 3 smd rect (at 0.762 -0.39878 270) (size 0.762 0.4318)
      (layers F.Cu F.Paste F.Mask)
      (net 38 N-000004)
    )
    (pad 6 smd rect (at -0.762 -0.39878 270) (size 0.762 0.4318)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 1 smd rect (at 0.762 1.19888 270) (size 0.762 0.4318)
      (layers F.Cu F.Paste F.Mask)
      (net 40 N-000005)
    )
    (pad 4 smd rect (at 0.762 -1.19888 270) (size 0.762 0.4318)
      (layers F.Cu F.Paste F.Mask)
      (net 27 N-0000015)
    )
    (pad 5 smd rect (at -0.762 -1.19888 270) (size 0.762 0.4318)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 8 smd rect (at -0.762 1.19888 270) (size 0.762 0.4318)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (model smd/resistors/r_cat16-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module crystal_smd_5x3.2mm (layer F.Cu) (tedit 52C3DF97)
    (at 119.0625 90.8685 90)
    (descr "5x3.2mm SMD glass Crystal")
    (fp_text reference X1 (at 0 -2 90) (layer F.SilkS) hide)
    (fp_text value 25MHz (at 0 2.1 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.85 0 90) (size 1.7 2.4)
      (layers F.Cu F.Paste F.Mask)
      (net 19 /XI)
      (solder_mask_margin 0.06858)
    )
    (pad 2 smd rect (at 1.85 0 90) (size 1.7 2.4)
      (layers F.Cu F.Paste F.Mask)
      (net 20 /XO)
      (solder_mask_margin 0.06858)
    )
    (model walter/crystal/crystal_smd_5x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lqfp48 (layer F.Cu) (tedit 52C3DFE5)
    (at 109.728 89.9795 270)
    (descr LQFP-48)
    (fp_text reference IC1 (at 0 1.143 270) (layer F.SilkS) hide)
    (fp_text value W5500 (at 0 -1.143 270) (layer F.SilkS) hide)
    (pad 4 smd rect (at -1.24968 4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (pad 5 smd rect (at -0.7493 4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 11 /RXN)
    )
    (pad 6 smd rect (at -0.24892 4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 12 /RXP)
    )
    (pad 7 smd rect (at 0.24892 4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 34 N-0000036)
    )
    (pad 8 smd rect (at 0.7493 4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (pad 1 smd rect (at -2.75082 4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 17 /TXN)
    )
    (pad 2 smd rect (at -2.25044 4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 18 /TXP)
    )
    (pad 3 smd rect (at -1.75006 4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 13 smd rect (at 4.09956 2.75082 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 30 N-0000031)
    )
    (pad 14 smd rect (at 4.09956 2.25044 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 15 smd rect (at 4.09956 1.75006 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (pad 16 smd rect (at 4.09956 1.24968 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 17 smd rect (at 4.09956 0.7493 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (pad 18 smd rect (at 4.09956 0.24892 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 35 N-0000037)
    )
    (pad 19 smd rect (at 4.09956 -0.24892 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 20 smd rect (at 4.09956 -0.7493 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 33 N-0000035)
    )
    (pad 25 smd rect (at 2.75082 -4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 3 /LNKLED)
    )
    (pad 26 smd rect (at 2.25044 -4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 29 N-000003)
    )
    (pad 27 smd rect (at 1.75006 -4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 2 /ACTLED)
    )
    (pad 28 smd rect (at 1.24968 -4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 29 smd rect (at 0.7493 -4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 30 smd rect (at 0.24892 -4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 19 /XI)
    )
    (pad 31 smd rect (at -0.24892 -4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 20 /XO)
    )
    (pad 32 smd rect (at -0.7493 -4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 21 /nCS)
    )
    (pad 37 smd rect (at -4.09956 -2.75082 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 23 /nRST)
    )
    (pad 38 smd rect (at -4.09956 -2.25044 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 8 /RSVD)
    )
    (pad 39 smd rect (at -4.09956 -1.75006 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 8 /RSVD)
    )
    (pad 40 smd rect (at -4.09956 -1.24968 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 8 /RSVD)
    )
    (pad 41 smd rect (at -4.09956 -0.7493 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 8 /RSVD)
    )
    (pad 42 smd rect (at -4.09956 -0.24892 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 8 /RSVD)
    )
    (pad 43 smd rect (at -4.09956 0.24892 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /PMODE0)
    )
    (pad 44 smd rect (at -4.09956 0.7493 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /PMODE0)
    )
    (pad 9 smd rect (at 1.24968 4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 10 smd rect (at 1.75006 4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 39 N-0000040)
    )
    (pad 11 smd rect (at 2.25044 4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (pad 12 smd rect (at 2.75082 4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 32 N-0000034)
    )
    (pad 21 smd rect (at 4.09956 -1.24968 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (pad 22 smd rect (at 4.09956 -1.75006 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 31 N-0000033)
    )
    (pad 23 smd rect (at 4.09956 -2.25044 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 9 /RSVD5)
    )
    (pad 24 smd rect (at 4.09956 -2.75082 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 26 N-0000014)
    )
    (pad 33 smd rect (at -1.24968 -4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 13 /SCK)
    )
    (pad 34 smd rect (at -1.75006 -4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 15 /SO)
    )
    (pad 35 smd rect (at -2.25044 -4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 14 /SI)
    )
    (pad 36 smd rect (at -2.75082 -4.09956 270) (size 0.29972 1.30048)
      (layers F.Cu F.Paste F.Mask)
      (net 22 /nINT)
    )
    (pad 45 smd rect (at -4.09956 1.24968 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /PMODE0)
    )
    (pad 46 smd rect (at -4.09956 1.75006 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 37 N-0000039)
    )
    (pad 47 smd rect (at -4.09956 2.25044 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 36 N-0000038)
    )
    (pad 48 smd rect (at -4.09956 2.75082 270) (size 1.30048 0.29972)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (model walter/smd_lqfp/lqfp-48.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module inductor_smd_0603 (layer F.Cu) (tedit 52C3E012)
    (at 103.9495 98.4885)
    (descr "Inductor SMD, 0603")
    (fp_text reference L1 (at 0 -1.09982) (layer F.SilkS) hide)
    (fp_text value INDUCTOR (at 0 1.19888) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.63754 0) (size 0.635 1.016)
      (layers F.Cu F.Paste F.Mask)
      (net 4 /NICAVDD)
    )
    (pad 2 smd rect (at 0.63754 0) (size 0.635 1.016)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (model walter/smd_inductors/inductor_smd_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3DFD8)
    (at 107.315 81.5975)
    (attr smd)
    (fp_text reference R13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 1 +3.3V)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 5 /PMODE0)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM0603 (layer F.Cu) (tedit 52C3DFE0)
    (at 107.315 83.3755)
    (attr smd)
    (fp_text reference R14 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 24 GND)
    )
    (pad 2 smd rect (at 0.762 0) (size 0.635 1.143)
      (layers F.Cu F.Paste F.Mask)
      (net 8 /RSVD)
    )
    (model smd\resistors\R0603.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 49.8475 (width 0.3) (layer Dwgs.User)
    (gr_text "49.847 mm" (at 105.50525 74.088) (layer Dwgs.User))
    (feature1 (pts (xy 130.429 79.5655) (xy 130.429 72.738)))
    (feature2 (pts (xy 80.5815 79.5655) (xy 80.5815 72.738)))
    (crossbar (pts (xy 80.5815 75.438) (xy 130.429 75.438)))
    (arrow1a (pts (xy 130.429 75.438) (xy 129.302496 76.024421)))
    (arrow1b (pts (xy 130.429 75.438) (xy 129.302496 74.851579)))
    (arrow2a (pts (xy 80.5815 75.438) (xy 81.708004 76.024421)))
    (arrow2b (pts (xy 80.5815 75.438) (xy 81.708004 74.851579)))
  )
  (dimension 20.828 (width 0.3) (layer Dwgs.User)
    (gr_text "20.828 mm" (at 137.3035 89.9795 270) (layer Dwgs.User))
    (feature1 (pts (xy 130.429 100.3935) (xy 138.6535 100.3935)))
    (feature2 (pts (xy 130.429 79.5655) (xy 138.6535 79.5655)))
    (crossbar (pts (xy 135.9535 79.5655) (xy 135.9535 100.3935)))
    (arrow1a (pts (xy 135.9535 100.3935) (xy 135.367079 99.266996)))
    (arrow1b (pts (xy 135.9535 100.3935) (xy 136.539921 99.266996)))
    (arrow2a (pts (xy 135.9535 79.5655) (xy 135.367079 80.692004)))
    (arrow2b (pts (xy 135.9535 79.5655) (xy 136.539921 80.692004)))
  )
  (gr_text 20140102 (at 100.711 81.2165) (layer B.Cu))
  (gr_text "5V\n\n3.3V" (at 123.3805 96.5835 90) (layer B.SilkS))
  (gr_text RSTN (at 110.9345 83.75 90) (layer B.SilkS))
  (gr_text INTN (at 113.4745 83.75 90) (layer B.SilkS))
  (gr_text SI (at 116.0145 83.75 90) (layer B.SilkS))
  (gr_text SO (at 118.5545 83.75 90) (layer B.SilkS))
  (gr_text SCK (at 121.0945 83.75 90) (layer B.SilkS))
  (gr_text CSN (at 123.698 83.75 90) (layer B.SilkS))
  (gr_text VCC (at 126.1745 83.75 90) (layer B.SilkS))
  (gr_text GND (at 128.651 83.75 90) (layer B.SilkS))
  (gr_text "W5500\nBREAKOUT\nver 1.0" (at 100.7745 81.3435) (layer F.SilkS))
  (gr_text "hairy.geek.nz\nCC BY-SA" (at 118.1735 83.947) (layer F.SilkS))
  (gr_line (start 80.6 79.6) (end 80.6 100.4) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80.6 100.4) (end 130.4 100.4) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.4 79.6) (end 130.4 100.4) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80.6 79.6) (end 130.4 79.6) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text 100 (at 127.5715 95.504) (layer F.SilkS))
  (gr_text LNK (at 127.508 98.044) (layer F.SilkS))
  (gr_text FDX (at 127.4445 92.964) (layer F.SilkS))
  (gr_text ACT (at 127.508 90.3605) (layer F.SilkS))
  (zone (net 24) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.581 77.7875) (xy 133.4135 77.7875) (xy 133.4135 102.6795) (xy 76.581 102.6795)
      )
    )
  )
  (zone (net 24) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.057 76.7715) (xy 131.953 76.708) (xy 131.826 105.029) (xy 74.7395 104.394)
      )
    )
  )
)
